{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Pót 1 ablakok Webra"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Pót 1 ablakok Webra","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sorszám","megnevezés","mennyiség","egység","anyag","díj","összes anyag","összes díj"]
[]
[1,"ÚJ alumínuim nyíló tetőablakok készítése 90*180 cm méretben motoros nyitással, az üveg tetőszerkezet átalakításával 3.3.1-16-3.3.1 AR Low-e üvegezéssel",32,"db",null,null,{"$f":"E6*C6","v":0},{"$f":"F6*C6","v":0}]
[2,"Szilárd tüzelésű kazánok kéményeinek átalakítása Proschorn DW-Alkon 300/360mm kéményekkel, szükséges idomokkal és tartószerkezettel",2,"db",null,null,{"$f":"E7*C7","v":0},{"$f":"F7*C7","v":0}]
[]
[]
[{"$nulls":6},{"$f":"SUM(G6:G7)","v":0},{"$f":"SUM(H6:H7)","v":0}]
[]
[{"$nulls":6},"összesen nettó",{"$f":"SUM(G10:H10)","v":0}]
[{"$nulls":6},"áfa",{"$f":"H12*0.27","v":0}]
[{"$nulls":6},"bruttó",{"$f":"H12+H13","v":0}]