{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["SZTE"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"SZTE","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[[14,1,14,6],[15,1,15,6],[14,7,14,8],[15,7,15,8],[13,7,13,8],[1,0,1,7],[12,1,12,6],[13,1,13,6]],"flags":["formulas_cached_only"]}
["Ssz.",null,"Típus, megnevezés","Menny.","Egység","Anyag egységár","Díj egységár","Anyag összesen","Díj  összesen"]
["JGYTF szercer1-szerver2 összekötése 8 szálas optikával"]
[1,null,"Nyomvonal építés 40x17-es csatornával",80,"m",0,0,0,0]
[2,null,"Optikai patch panel",2,"db",0,0,0,0]
[3,null,"Optikai kábel kikötése patch panelra SC",16,"db",0,0,0,0]
[4,null,"Duplex multimódusú patchkábel 50/125µm (OM3), 2xLC-2xSC, 2 m",2,"db",0,0,0,0]
[5,null,"Optikai kábel 8x50/125 OM3",100,"m",0,0,0,0]
[6,null," mérés",16,"db",0,0,0,0]
[7,null,"10/100/1000Base-T to 1000Base-SX Gigabit Converter",2,"db",0,0,0,0]
[8,null,"Cat.5E UTP kábel telefonnak LSOH",90,"m",0,0,0,0]
[9,null,"Telefon kábel kikötése meglévő patch panelra",2,"db",0,0,0,0]
[10,null," mérési jegyzőkönyvek készítése",1,"ö",0,0,0,0]
[11,"Nettó összesen:",{"$nulls":5},0,0]
[12,"Nettó összesen (anyag + díj):",{"$nulls":5},0]
[13,"ÁFA",{"$nulls":5},0]
[14,"Mindösszesen",{"$nulls":5},0]