{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Munka1","Munka2","Munka3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[8,0,13,0],[8,1,13,1]]}
[]
[null,null,null,"SZTE/2015/PB05944"]
[null,null,null,"Specifikáció - laboratóriumi eszközök 4 részajánlati körben"]
[]
[null,"Név","Db","Specifikáció","Típus","Megjegyzés"]
["1. részajánlati kör","Gél ElFo1",1,"ELECTROPHORESIS UNIT MINI VERT SE250 COM 0,75MM Complete system includes lower buffer chamber, upper buffer chamber/cooling core, safety lid with high voltage leads, casting cradle with sealing gasket set, 2× casting clamp assemblies, 4× cams, 10× rectangular glass plates (10×8 cm), 5× alumina plates, notched (10×8 cm), 4× spring clamps, 2× combs (10-well, 0,75 mm thickness), 4× T-spacers (0,75 mm thickness), 2× well locating decals, and gel seal. SUBMARINE ELECTROPHOR UNIT HOR SUB6, SPACER T-SHAPE 8CM X 1,0MM, SPACER T-SHAPE 8CM X 1.5MM, COMB SPINELESS 10 WELL 1MM, COMB SPINELESS 10 WELL 1.5MM, PLATE ALUMINA 10X8CM NOTCHED, PLATE GLASS 10X8CM RECTANGULAR.","ELECTROPHORESIS UNIT MINI VERT SE250 COM 0,75MM, kiegészítőkkel"]
["2. részajánlati kör","Gél ElFo2",1,"ELECTROPHORESIS UNIT MINI VERT SE260 COM 0,75MM Complete system includes  Lower Buffer Chamber,  Upper Buffer Chamber/Cooling Core; \nSafety Lid with High Voltage Leads; Casting Cradle w/Sealing Gasket Set; Casting Clamp Assemblies-2 pcs, Cams-4 pcs; Glass Plates, Rectangular, 10 x 10.5 cm-10 pcs; Alumina Plates, Notched, 10 x 10.5 cm-5 pcs; Spring Clamps-4 pcs; Combs, 10 well-2 pcs; T-Spacers-4 pcs; Well Locating Decals-2 pcs; Gel Seal; Gel plate size 10 × 10.5 cm; Max. wattage 12 W; Max. voltage 500 V; Max. amperage 500 mA; Max. temperature 45 °C; Dimensions (w × h × d) 16.5 × 16 × 16 cm; PLATE GLASS 10X8CM RECTANGULAR; PLATE ALUMINA 10X8CM NOTCHED; SPACER T-SHAPE 8CM X 0,75MM; SPACER T-SHAPE 8CM X 1,0MM; SPACER T-SHAPE 8CM X 1,5MM; SPACER T-SHAPE 10,5CM X 1MM; SPACER T-SHAPE 10,5CM X 1,5MM; COMB SPINELESS 5 WELL 1,5MM; COMB SPINELESS 10 WELL 1MM; COMB SPINELESS 10 WELL 1,5MM; COMB SPINELESS 12 WELL 1MM; COMB SPINELESS 15 WELL 1,5MM.","ELECTROPHORESIS UNIT MINI VERT  SE260-10A-0,75MM, kiegészítőkkel"]
["3. részajánlati kör","Vízfürdő",2,"Max. 100 ºC-ig, Fenéklemezzel és kúpos tetővel, Külső méret: szél x mélység x mag : 685 x 440 x 255 mm, Belső méret: szél x mélység x mag : 600 x 245 x 145 * mm, Átfolyóvíz szintszabályozó kittel,a vízhőfok + 3 °C-tól állítható, Mikroprocesszoros kontroll, Digitális hőmérséklet kijelzés (0,1 ˚C), Gyors felfűtés – teljesítmény: 1500 W, Rozsdamentes acél kivitel. Fedőlemez és a perforált fenéklemez standard felszereltség, Kettős túlfűtés elleni védelem, Vízhiány (alacsony víz, elpárolgás) esetén automatikus kikapcsolás ","GFL 1004 Vízfürdő, 21 literes","Kérjük, hogy  csak a kiírásban meghatározott termékre, vagy ezzel műszaki tartalmában teljesen egyenértékű helyettesítő termékre adjon be ajánlatot!"]
["4. részajánlati kör","Pipetták",2,"PIPETMAN G P2G . METAL EJECTOR 0.2-2uL","Gilson"]
[null,null,3,"PIPETMAN G P20G . METAL EJECTOR 2-20uL","Gilson"]
[null,null,3,"PIPETMAN G P200G . METAL EJECTOR 20 -200uL","Gilson"]
[null,null,3,"PIPETMAN G P1000G . METAL EJECTOR 100 -1000uL","Gilson"]
[null,null,2,"PIPETMAN G P5000G 500 -5000uL","Gilson"]
[null,null,1,"Pipetta 12-csatornás mechanikus, 30-300ul, autoklávozható, narancs.","Eppendorf Research Plus"]

{"sheet":"Munka2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Munka3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}