{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["SZTE"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"SZTE","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[[13,1,13,6],[14,1,14,6],[13,7,13,8],[14,7,14,8],[12,7,12,8],[1,0,1,7],[11,1,11,6],[12,1,12,6]],"flags":["formulas_cached_only"]}
["Ssz.",null,"Típus, megnevezés","Menny.","Egység","Anyag egységár","Díj egységár","Anyag összesen","Díj  összesen"]
[]
[1,null,"Nyomvonal építés csatornával, szükség esetén faláttöréssel, javítással",200,"m",0,0,0,0]
[2,null,"1U 19\" patch panel Cat. 5e 24xRJ45/s",1,"db",0,0,0,0]
[3,null,"UBIQUITI UAP-AC-PRO",24,"db",0,0,0,0]
[4,null,"HP2530-24G-POE Switch+ szoftver",1,"db",0,0,0,0]
[5,null,"Csatlakozó modul Cat. 5e 24xRJ45/s",24,"db",0,0,0,0]
[6,null,"Patch cord R&M freenet Cat.5 SF-UTP 4P 1m",48,"db",0,0,0,0]
[7,null,"Cat.5E F/UTP 4P LSOH kábel",1440,"m",0,0,0,0]
[8,null,"Falon kívüli aljzat 2x1 port, fehér+(vak védő)",24,"db",0,0,0,0]
[9,null," mérési jegyzőkönyvek készítése (végpontok)",24,"db",0,0,0,0]
[10,"Nettó összesen:",{"$nulls":5},0,0]
[11,"Nettó összesen (anyag + díj):",{"$nulls":5},0]
[12,"ÁFA",{"$nulls":5},0]
[13,"Mindösszesen",{"$nulls":5},0]