{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tűzjelző rendszer - I.em."],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":9,"defined_names":55,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tűzjelző rendszer - I.em.","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[[15,1,15,3],[19,1,19,2],[14,1,14,3],[13,1,13,3],[0,0,0,1],[8,0,8,1],[12,1,12,3],[2,0,2,9],[10,0,10,9]],"flags":["formulas_cached_only"]}
["Megnevezés",null,"Típus","Műszaki tartalom","Mennyiség","M.e.","Anyag egység","Díj egység","Anyag összes","Díj összes"]
[]
["Eszközök, berendezések"]
[]
[1,"Szerelő doboz","A11 kötődoboz","85 x 85 x 40 mm, IP54",86,"db",0,0,0,0]
[]
[{"$nulls":7},"Összesen:",0,0]
[]
["Megnevezés",null,"Típus","Műszaki tartalom","Mennyiség","M.e.","Anyag egység","Díj egység","Anyag összes","Díj összes"]
[]
["Vezetékhálózat kiépítése"]
[]
[1,"átm. 20mm MÜ II Védőcső  horony véséssel, helyreállítással",null,null,604,"m",0,0,0,0]
[2,"átm. 20mm MÜ II Védőcső  horony véséssel, helyreállítással RWA részére",null,null,58,"m",0,0,0,0]
[2,"Tűzgátló falátvezetés készítése",null,null,3,"klt",0,0,0,0]
[3,"Egyéb szerelési anyag",null,null,1,"klt",0,0,0,0]
[]
[{"$nulls":7},"Összesen:",0,0]
[]
[null,"Összesítés:"]
[null,"Anyag:",0]
[null,"Díj:",0]
[null,"Nettó:",0]