{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Összesítés"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Összesítés","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["GINOP-2.3.2-15-2016-00013"]
["Funkcionális felületeken alapuló intelligens anyagok – az előállítástól az alkalmazásokig"]
[]
["Sorsz.","Megnevezés","minőség","m3/kg","űrtartalom","Igényelt mennyiség","Megjegyzés"]
["1.","Szintetikus levegő","ipari","6 m3","40 L",30]
["2.","Szintetikus levegő","ipari","1,5 m3","14 L",10]
["3.","Szén-dioxid","élelmiszerip.","20 kg","27 L",1]
["4.","Oxigén","ipari","1,5 m3","10 L",5]
["5.","Nitrogén","5.0","6 m 3","40 L",2]
["6.","Nitrogén","4.5","6 m 3","40 L",25]
["7.","Nitrogén","4.5","1.5m 3","10 L",10]
["8.","Hidrogén","ipari","6 m3","40 L",5]
["9.","Hidrogén","5.0","10 m 3","50 L",3]
["10.","Hélium","4.6","6 m3","40 L",1]
["11.","Hélium","6.0","10 m3","50 L",2]
["12.","Argon","4.6","6 m3","40 L",6]
["13.","Argon","4.6","10 m3","50 L",5]
["14.","Disszugáz","2.6","6 kg","40 L",5]
["15.","Szárazjég  3mm, 16 mm",null,"kg",null,3]
["16.","Ammónia","ipari","20 kg","40 L",1]
["17.","Metán","4.5","12 m3","50 L",1]
["18.","Palack reduktor ipari 200/10 bar","4.8 -ig",null,null,2,"Argon gázpalackhoz"]
["19.","Reduktor tömítés",null,null,null,30]
["20.","Etilén","3.0",null,"10 L",5]