{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":13,"n_cols":8,"rows_kept":13,"cut":false,"hidden":false,"merged":[[12,6,12,7]]}
[null,null,"KÖLTSÉGVETÉS"]
[]
[null,"Károlyi Mihály Kollégium biztonsági világítás javítás"]
[]
["Ssz.","Tétel szövege","Menny.","Egység","Anyag egységár","Díj egységre","Anyag összesen","Díj összesen"]
[1,"2x18 W-os inverteres lámpastest",2,"db",null,null,{"$f":"ROUND(C6*E6, 0)","v":0},{"$f":"ROUND(C6*F6, 0)","v":0}]
[2,"Akkumulátor 4,8 V, 1,5 A",45,"db     ",null,null,0,0]
[3,"Akkumulátor 3,6 V, 1,5 A",35,"db",null,null,0,0]
[4,"Érintésvédelmi mérés és jegyzőkönyv készítése",1,"klt",null,null,{"$f":"ROUND(C9*E9, 0)","v":0},{"$f":"ROUND(C9*F9, 0)","v":0}]
[]
[null,"ÖSSZESEN:",{"$nulls":4},{"$f":"SUM(G6:G10)","v":0},{"$f":"SUM(H6:H10)","v":0}]
[]
[null,"ANYAG+DÍJ ÖSSZESEN",{"$nulls":4},{"$f":"G11+H11","v":0}]