{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Munka1","Munka2","Munka3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":26,"n_cols":3,"rows_kept":26,"cut":false,"hidden":false,"merged":[[6,1,6,2],[16,1,16,2],[5,1,5,2],[3,1,3,2]]}
[]
[null,"SZTE/2014/PB03779"]
[]
[null,"Szűrőbeszerzés - specifikáció"]
[]
[null,"SZTE TIK  11 db légtechnikai géphez 162 db szűrő típus és méret szerint:"]
[null,"Szűrő típusa: G4"]
[null,"mérete:                                                            szélesség x magasság x zsák mélység","db"]
[null,"592x592x365 ",57]
[null,"592x287x356",11]
[null,"287x592x356",19]
[null,"287x287x356  ",11]
[null,"490x592x356",8]
[null,"492x592x356",1]
["Összesen: ",null,{"$f":"SUM(C9:C14)","v":107}]
[]
[null,"Szűrő típusa: F7"]
[null,"mérete:                                                            szélesség x magasság x zsák mélység"," db"]
[null,"592x592x610",29]
[null,"592x287x610",6]
[null,"287x592x610",10]
[null,"287x287x610    ",6]
[null,"490x592x610",4]
["Összesen: ",null,{"$f":"SUM(C19:C23)","v":55}]
[]
[null,"A két típus összesen:",{"$f":"C15+C24","v":162}]

{"sheet":"Munka2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Munka3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}