{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":13,"n_cols":8,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
[{"$nulls":4},"KÖLTSÉGVETÉS"]
[]
[null,null,"SZTE Igazgatásszervezési és Szolgáltatási Központ"]
[null,null,"Szünetmentes tápegység akkumulátor cseréje"]
[]
["S.sz.","Megnevezés","Menny.","Me","Anyag:","Díj:","Anyag Ö.:","Díj Ö.:"]
[]
[1,"DSP Multipower 6kVA PM sszünetmentes tápegység akkumulátor cseréje. AC INPUT: 180V-280V,  30A Max 50/60 Hz, AC OUTPUT: 220V 50/60 Hz P: 6000 VA/4800 W, PF=0,8",1,"klt"]
[]
[2,"Üzembe helyezés",1,"alk"]
[3,"Kiszerelt akkumlátorok elszállítása, bizonylatolással ",1,"klt"]
[null,"Összesen:",{"$nulls":4},{"$f":"SUM(G9:G11)","v":0},{"$f":"SUM(H9:H12)","v":0}]