{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Árazatlan k."],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Árazatlan k.","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,6,0,7],[5,1,6,1],[5,0,6,0],[5,2,5,4],[5,5,5,6],[5,7,6,7],[2,0,2,7],[4,0,4,7],[21,0,21,7],[23,0,23,7],[17,0,17,4],[18,0,18,4],[19,0,19,4],[17,5,17,7],[18,5,18,7],[19,5,19,7],[22,0,22,3]],"flags":["formulas_cached_only"]}
[]
[]
["KÖLTSÉGVETÉS"]
[]
["Sebészeti Műtéttani Intézet ATS riasztó rendszerének bővítése"]
["Típus/\nGyártó","Leírás:","Anyagköltség:",null,null,"Munkadíj:",null,"Összesen:"]
[null,null,"Meny-nyiség:","Egység-ár:","Összesen:","Egység-ár:","Összesen:"]
["ATS 1115","Portai LCD kezelő",1,null,0,null,null,0]
["DC 143","Nyitásérzékelő",2,null,0,null,null,0]
["ATS-RF","Nyitásérzékelő",8,null,0,null,null,0]
["VE 1120","Mozgásérzékelő",2,null,0,null,null,0]
["ATS-RF","Mozgásérzékelő",1,null,0,null,null,0]
["ATS-RF","Zónabővítő",2,null,0,null,null,0]
["ATS 1201E","Zónabővítő",2,null,0,null,null,0]
["ATS 1160N","Kártyaolvasó",1,null,0,null,null,0]
["12V/18Ah","Akkumulátor",2,null,0,null,null,0]
[null,"Kábelek, segédanyagok",1,null,0,null,null,0]
["Összesen anyagköltség (nettó):",{"$nulls":4},0]
["Összesen munkadíj (nettó):"]
["Mindösszesen (nettó):",{"$nulls":4},0]
[]
["A fenti megadott típusoktól el lehet térni, amennyiben a kiadott módosított műszaki leírás szerinti feladat teljesíthető."]