{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Munka1","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,2,1,6],[6,2,6,6],[15,2,15,5],[7,7,7,8],[7,9,7,10],[2,2,2,6],[3,2,3,6]]}
["1.részajánlati kör:  Szonotródák "]
["S.szám","Megnevezés","Specifikáció",{"$nulls":4},"Kiszerelés",null,"Igényelt mennyiség"]
["1.","Szonotróda ","Titánból készült Ø 10mm Hossz: kb. 100mm, 50ml-től 1000ml minta térfogatig",{"$nulls":4},1,"db",2,"db"]
["2.","Szonotróda ","Titánból készült Ø 5mm Hossz: kb. 100mm, 20ml-től 300ml minta térfogatig",{"$nulls":4},1,"db",2,"db"]
[]
["2.részajánlati kör: Üvegcsiszolatok, szűrőlap, tefloncsap: "]
["S.szám","Megnevezés","Specifikáció",{"$nulls":4},"Kiszerelés",null,"Igényelt mennyiség"]
[null,null,"Méret","Hossz (mm)","Fal vastagság (mm)","Külső cső átmérő (mm)","Egyébb"]
[1,"Csiszolat hüvely","NS 10/19","130±50","1,5±0,5","13±1","üveg",1,"db",20,"db"]
[2,"Csiszolat hüvely","NS 29/32","130±50","2,0±0,5","33±3","üveg",1,"db",20,"db"]
[3,"Csiszolat dugó","NS 10/19","115±50","1,5±0,5","8±3","üveg",1,"db",20,"db"]
[4,"Csiszolat dugó","NS 14/23","130±50","1,5±0,5","13±1","üveg",1,"db",20,"db"]
[5,"Csiszolat dugó","NS 19/26","130±50","1,8±0,5","17±2","üveg",1,"db",20,"db"]
[6,"Csiszolat dugó","NS 24/29","130±50","1,8±0,5","22±2","üveg",1,"db",20,"db"]
[7,"Csiszolat dugó","NS 29/32","130±50","2,0±0,5","26±2","üveg",1,"db",20,"db"]
[8,"Szűrőlap","P3, 25 mm átmérő",null,null,null,"üveg",1,"db",20,"db"]
[9,"Teflon csap","Lyukátmérő 0-4,0 mm, 8-as szárral",null,null,null,"üveg, PTFE",1,"db",15,"db"]